Moonlite 80 Flush mount bracket installation procedure

A speaker on a shelf

Description automatically generated with low confidenceA picture containing weapon, ground

Description automatically generatedRemove bracket from wrapping

With a deep 7mm socket remove and discard the 4 nyloc nuts

A picture containing indoor, black, kitchenware, pan

Description automatically generated

Unscrew the 4 screws completely so the facia panel is now apart from the retaining sectionA picture containing ground, outdoor, silver

Description automatically generated

With the 4 short screws supplied fix the facia panel to the Moonlite 80 and secure tight also completely remove the hanging bracket of the Moonlite 80 and discard

A picture containing electronics, black, camera lens

Description automatically generatedA picture containing leather, close

Description automatically generatedA picture containing floor, indoor

Description automatically generated

Now drill 160mm diameter hole in the surface you plan to install the fixture into

A picture containing indoor, measuring stick

Description automatically generated

Now feed the retaining section of the bracket through the 160mm hole ensuring it is perfectly placed in the centre of the hole

A circular object on a white surface

Description automatically generated with low confidence

Complete your wiring of the fixture via the hole connect power and data to the Moonlite 80 and install and secure the Moonlite 80 with the 4 long screws to the retaining section.

A picture containing indoor

Description automatically generatedA picture containing indoor

Description automatically generated

A close up of a speaker

Description automatically generated with medium confidenceInstallation complete